#
EMISSION SYSTEM LOCATION INDEX

id011600803700

Engine room side

Fuel tank side

1 | PCV valve (See PCV VALVE INSPECTION)
2 | Purge solenoid valve (See PURGE SOLENOID VALVE REMOVAL/INSTALLATION) (See PURGE SOLENOID VALVE INSPECTION)
3 | Charcoal canister (See CHARCOAL CANISTER REMOVAL/INSTALLATION) (See CHARCOAL CANISTER INSPECTION)
4 | Quick release connector (See FUEL HOSE (FUEL TANK SIDE) REMOVAL/INSTALLATION)
5 | Evaporative gas check valve (two-way) (See EVAPORATIVE GAS CHECK VALVE (TWO-WAY) REMOVAL/INSTALLATION) (See EVAPORATIVE GAS CHECK VALVE (TWO-WAY) INSPECTION)
6 | Rollover valve (See ROLLOVER VALVE REMOVAL/INSTALLATION) (See ROLLOVER VALVE INSPECTION)