#
THROTTLE BODY CONSTRUCTION [L8, LF, L3]

id0113z1147700
• The throttle body mainly consists of the throttle valve, TP sensor, and throttle actuator.
• A low-energy consuming DC motor has been adopted for the throttle actuator to improve response performance.
• To keep moisture from freezing inside the throttle body, and thus prevent the throttle valve from getting stuck, engine coolant is circulated through the throttle body.
• To prevent the possible loss of PCM data and throttle body settings, the throttle body cannot be disassembled.