#
FRONT BRAKE (DISC) REMOVAL/INSTALLATION [18 INCH WHEEL]

id0411008009b3

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

3. After installation, depress the pedal a few times, rotate the wheel by hand, and verify that the brake does not drag.

.

1 | Brake hose
2 | Retaining clip (See Retaining Clip Installation Note.)
3 | Cap
4 | Bolt
5 | Caliper
6 | Boot
7 | Disc pad (See Disc Pad Installation Note)
8 | Bolt
9 | Mounting support
10 | Disc plate (See Disc Plate Removal Note) (See Disc Plate Installation Note)

## Disc Plate Removal Note

1. Mark the wheel hub bolt and disc plate before removal for reference during installation.

## Disc Plate Installation Note

1. Remove any rust or grime on the contact face of the disc plate and wheel hub.

2. Install the disc plate and align the marks made before removal.

## Disc Pad Installation Note

1. Push the piston fully inward using the SST.

2. Install the disc pad.

## Retaining Clip Installation Note

1. Temporarily install the retaining clip to the caliper and mounting support as shown in the figure.

2. Secure the retaining clip so that part A does not slip off from the caliper while installing part B to the mounting support.

3. Verify that the retaining clip is securely installed to the caliper and the mounting support.