CYLINDER HEAD ASSEMBLY (I)

id011000504300

1. Disassemble in the order indicated in the table.

beltze00000087

1 | Water outlet case
2 | Valve seal (See Valve Seal Assembly Note.)
3 | Valve
4 | Valve spring
5 | Upper valve spring seat
6 | Valve keeper (See Valve Keeper Assembly Note.)
7 | Engine hanger

Water Outlet Case Assembly Note

1. Tighten the bolts in the order shown in the figure.

beltze00000088

Valve Seal Assembly Note

1. Press in the valve seal to the valve guide by hand.

2. Install the valve seal using the SST.

beldje00000215

Valve Keeper Assembly Note

1. Assemble the valve keeper using the SST.

beltze00000089