#
FEEDBACK CONTROL STRUCTURE [FS5A-EL]

id051721111800

## Features

• Regulation of hydraulic pressure for engagement and disengagement is optimized through feedback and learning correction of the clutch engagement pressure.

## Structure

Block diagram

.

1 | TFT sensor
2 | Input/turbine speed sensor
3 | Intermediate sensor
4 | Oil pressure switch
5 | MAF sensor
6 | Shift solenoid A
7 | Shift solenoid B
8 | Shift solenoid C
9 | Pressure control solenoid B