#
SOLENOID VALVE FUNCTION [JA5AX-EL]

id051705693100

.

1 | Shift solenoid C
2 | High clutch solenoid valve
3 | 2-4 brake solenoid valve
4 | neutral shift solenoid valve
5 | Shift solenoid B
6 | Reduction timing solenoid valve
7 | Shift solenoid A
8 | Torque converter solenoid valve
9 | Pressure control solenoid

Function chart

Solenoid | Type | Characteristics | Function
--- | --- | --- | ---
Pressure control solenoid | Repeats ON and OFF at 50 Hz (20 ms cycle); duty cycle type (three-way type) | Normal high | Controls pressure regulator valve, regulates line pressure
Torque converter clutch (TCC) solenoid valve | Normal low | Controls TCC engagement and disengagement
2-4 brake solenoid valve | Normal high | Control 2-4 brake engagement and disengagement
High clutch solenoid valve | Control high clutch engagement and disengagement
Shift solenoid A | ON/OFF (three-way type) | Normal low | Control shift valve A
Shift solenoid B | Control shift valve B
Shift solenoid C | Control shift valve C
Reduction timing solenoid valve | ON/OFF (two-way type) | Control reduction reducing valve
Neutral shift solenoid | Control neutral shift valve and reverse inhibitor valve