#
JOINT SHAFT DISASSEMBLY [MZR-CD (RF Turbo)]

id0313008010j5

1. Disassemble in the order indicated in the table.

1 | Dust seal (wheel side)
2 | Snap ring (inner side)
3 | Snap ring (outer side)
4 | Joint shaft (See Joint Shaft Disassembly Note)
5 | Bearing (See Bearing, Dust Seal (Differential Side) Disassembly Note)
6 | Dust seal (differential side) (See Bearing, Dust Seal (Differential Side) Disassembly Note)
7 | Bracket

## Joint Shaft Disassembly Note

1. Disassemble the joint shaft using the SST.

## Bearing, Dust Seal (Differential Side) Disassembly Note

1. Remove the bearing and the dust seal (differential side) using the SSTs.