#
CLUTCH MASTER CYLINDER DISASSEMBLY/ASSEMBLY [L8, LF, L3]

id0510008023a4

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

1 | Clip
2 | Hose
3 | Joint
4 | Bushing
5 | Snap ring (See Snap Ring Disassembly/Assembly Note.)
6 | Piston and secondary cap component
7 | Spacer
8 | Primary cap
9 | Return spring
10 | Clutch master cylinder body

## Snap Ring Disassembly/Assembly Note

1. Hold the piston down using a cloth-wrapped pin punch.

  • If disassembling, remove the snap ring; if assembling, install it.