#
CLEARING CARD KEY [WITH ADVANCED KEYLESS SYSTEM]

id0914z68072b2

1. Fully lower the driver-side door glass.

2. Connect the WDS or equivalent to the DLC-2.

3. Pull out the WDS or equivalent cable from the door glass opening and set the WDS or equivalent outside the vehicle.

  Caution

  • Protect the cable and body contact area with a clean rag, otherwise they could be damaged.

4. Select "BODY/SECURITY/PATS (immobilizer)" from the WDS or equivalent screen menu.

5. Security access begins and the WDS or equivalent displays the "OUT-CODE".

  Note

  • When "OUT-CODE" is first displayed, turning the ignition switch from the LOCK to the ON position 5 times will change the "OUT-CODE".

6. Input the "IN-CODE" that corresponds to the "OUT-CODE" displayed in the WDS or equivalent screen.

7. Select "CARD KEY CLEARING" from the WDS or equivalent screen menu.