#
DSC OFF SWITCH REMOVAL/INSTALLATION

id041500801900

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | DSC OFF switch (See DSC OFF Switch Removal Note)
2 | Connector

3. Install in the reverse order of removal.

## DSC OFF Switch Removal Note

1. Insert your hand from the lower side of the dashboard and squeeze the tabs of the DSC OFF switch.

2. Pull the DSC OFF switch forward to remove it.