#
DISC PAD (REAR) REPLACEMENT [EXCEPT 18 INCH WHEEL]

id0411008003b4

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

.

1 | Parking brake cable, clip
2 | Bolt
3 | Caliper
4 | Spring
5 | Disc pad (See Disc Pad Installation Note.)
6 | Shim
7 | Guide plate

## Disc Pad Installation Note

1. Push the piston fully inward using the SST.

2. Install the disc pad.