#
NO.2 CASSETTE TAPE PLAYER DOES NOT EJECT THE CASSETTE TAPE

id0903a1805100

2 | Cassette tape player does not eject the cassette tape./00:Er01, 00:Er04, 00:Er10
TROUBLESHOOTING HINTS • Cassette tape is malfunctioning. • Cassette tape player is malfunctioning. • Cassette patch is broken. • Poor installation of cassette patch.

  Note

  • The cassette tape player may not eject the cassette tape due to the tape slack, peel-off or seal on it.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Click the eject button on the player. • Is "TAPE OUT" message displayed? | Yes | Go to the next step.
No | Replace the cassette patch.
2 | • Visually inspect the dust cover on the cassette patch. • Is there any damage on the cover? | Yes | Replace the cassette patch.
No | Go to the next step.
3 | • Inspect the cassette patch installation. • Is the cassette patch installed securely? Note • Inspect the connector for poor connection (such as damaged/bent/pulled-out pins, corrosion). | Yes | Replace the cassette tape player. Note When replacing the cassette tape player, inspect the followings: • No peeling-off the label. • Cassette patch is normal.
No | Install the cassette patch securely. If the cassette patch is broken, replace the cassette patch.