#
DTC B1134 [ADVANCED KEYLESS SYSTEM]

id0902e2350600

DTC B1134 | Unprogrammed card key.
--- | ---
POSSIBLE CAUSE | • Unprogrammed card key. • Malfunction in the keyless control module internal circuit

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY NUMBER OF REGISTERED CARD KEYS • Using the WDS or equivalent, perform the PID/data monitor inspection and confirm the number of registered keys. (See PID/DATA MONITOR TABLE [ADVANCED KEYLESS SYSTEM].) • Is card key registered? | Yes | Replace the keyless control module and perform the resetting procedure for the advanced keyless system when replacing the keyless control module. (See KEYLESS CONTROL MODULE REMOVAL/INSTALLATION [WITH ADVANCED KEYLESS SYSTEM].) (See CARD KEY ID CODE REGISTRATION [WITH ADVANCED KEYLESS SYSTEM]) (See STEERING LOCK UNIT ID CODE REGISTRATION [WITH ADVANCED KEYLESS SYSTEM]) (See KEYLESS CONTROL MODULE CONFIGURATION [WITH ADVANCED KEYLESS SYSTEM]) (See IMMOBILIZER SYSTEM COMPONENT REPLACEMENT/KEY ADDITION AND CLEARING [WITH ADVANCED KEYLESS SYSTEM]) (See SECURITY ACCESS PROCEDURE)
No | • Using the WDS or equivalent, register a card key if necessary. (See CARD KEY ID CODE REGISTRATION [WITH ADVANCED KEYLESS SYSTEM]) • Go to the next step.
2 | INSPECT KEYLESS CONTROL MODULE • Turn the ignition switch to the ON position. • Is the DTC displayed? - WDS or equivalent: B1134 | Yes | Replace the keyless control module and perform the resetting procedure for the advanced keyless system when replacing the keyless control module. (See KEYLESS CONTROL MODULE REMOVAL/INSTALLATION [WITH ADVANCED KEYLESS SYSTEM].) (See CARD KEY ID CODE REGISTRATION [WITH ADVANCED KEYLESS SYSTEM]) (See STEERING LOCK UNIT ID CODE REGISTRATION [WITH ADVANCED KEYLESS SYSTEM]) (See KEYLESS CONTROL MODULE CONFIGURATION [WITH ADVANCED KEYLESS SYSTEM]) (See IMMOBILIZER SYSTEM COMPONENT REPLACEMENT/KEY ADDITION AND CLEARING [WITH ADVANCED KEYLESS SYSTEM]) (See SECURITY ACCESS PROCEDURE)
No | DTC troubleshooting completed.