#
CABIN CONSTRUCTIOIN

id091000100700
• The floor, the side frame and the roof form three rigid, H-shaped frames (triple-H structure) that resist impact forces in the event of a side collision.
• Handling stability is improved by preventing body torsion.

.

1 | Roof reinforcement
2 | B-pillar
3 | Side sill
4 | Crossmember No. 2
5 | Crossmember No. 3
6 | Front door impact bar
7 | Rear door impact bar
8 | Collision energy