#
LINE PRESSURE CONTROL OUTLINE [JA5AX-EL]

id051705108200

## Features

• Line pressure is hydraulic pressure for operating friction elements such as the multiple disc clutches, multiple disc brakes, and the brake band.
• To adjust to optimal line pressure according to engine load conditions and vehicle driving conditions, continuous variable line pressure control from the pressure control solenoid is used.
• The line pressure control includes the basic control, line pressure control when shifting, backup control, and other.

## Construction (System Diagram)

.

1 | Intermediate sensor
2 | VSS
3 | Input/turbine speed sensor
4 | Throttle position signal
5 | Engine torque signal
6 | TFT sensor
7 | TCM
8 | TR switch
9 | Pressure control solenoid
10 | M range switch
11 | Up switch
12 | Down switch
13 | Cruise control module