#
CAR-NAVIGATION UNIT REMOVAL/INSTALLATION

id092000801000

1. Disconnect the negative battery cable.

2. Remove the glove compartment.

3. Remove in the order indicated in the table.

1 | Bolt
2 | Car-navigation unit (See Car-navigation Unit Installation Note)
3 | Connector

4. Install in the reverse order of removal.

## Car-navigation Unit Installation Note

1. Insert the car-navigation unit bracket into the dashboard member hole, and with the car-navigation unit fixed in place install the bolt.