#
CALIPER (REAR) DISASSEMBLY/ASSEMBLY [18 INCH WHEEL]

id0411008006b3

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

.

1 | Bleeder cap
2 | Bleeder screw
3 | Piston (See Piston Disassembly/Assembly Note)
4 | Piston boot
5 | Piston seal (See Piston Seal Disassembly Note.)
6 | Bracket
7 | Caliper body

## Piston Disassembly/Assembly Note

• Remove/install the piston using the SST.