#
OXIDATION CATALYTIC CONVERTER CONSTRUCTION [MZR-CD (RF Turbo)]

id0116f1156300
• The catalytic converter consists of an oxidation catalyst, diesel particulate filter, and an insulator which prevents heat damage around the converter.
• Inside the catalytic converter, monolith type catalyst has been adopted in which the oxidation catalyst and diesel particulate filter are independent.
• A cordierite oxidation catalyst has been adopted with a platinum coated surface.

.

1 | Oxidation catalytic converter
2 | Diesel particulate filter