#
REAR CROSSMEMBER OUTLINE

id021400111900
• The rear crossmember main frame is made from a steel pipe, improving strength without increasing weight.
• To reduce the noise from the suspension system to the body, rubber mounts are used at the four connecting points of the rear crossmember to the body.
• The construction of the rear crossmember mounting bushings are same as that of the front crossmember mounting bushings.