#
NO.3 CASSETTE TAPE PLAYER DOES NOT LOAD THE CASSETTE TAPE

id0903a1825500

3 | Cassette tape player does not load the cassette tape./00:Er01, 00:Er10
TROUBLESHOOTING HINTS • Cassette tape is malfunctioning. • Cassette tape player is malfunctioning. • Cassette patch is broken. • Poor installation of cassette patch. • Poor connection of cassette tape player connector.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Visually inspect the cassette tape. • Is the cassette tape normal? | Yes | Go to the Step 3.
No | Go to the next step.
2 | • Inspect the cassette tape player connector. • Does the cassette tape player load the cassette tape after-connecting the connector? | Yes | The cassette tape player is normal. Explain the repairs to the customer.
No | Replace the cassette tape player.
3 | • Replace with the cassette tape known to be good. • Does the cassette tape player load the cassette tape? | Yes | The cassette tape player is normal. Explain to the customer that the cassette tape is malfunctioning.
No | Go to the next step.
4 | • Visually inspect the duct cover on the cassette patch (damaged, crack, etc.). • Is the dust cover normal? | Yes | Replace the cassette tape player.
No | Replace the cassette patch.