#
DRIVE INFORMATION SYSTEM OPERATION

id092200111200

## Drive Information System Switch

• The drive information system switch comprises an INFO switch.
• The modes can be charged in a cyclic pattern by pressing the INFO switch.

• The data displayed at the time can be reset by holding the INFO switch for 1 second or more. Data are calculated as soon as the INFO switch is released.

## Drive Information System Display

• The display changes for each mode as shown.

Market | Instant fuel economy | Average fuel economy | Distance to empty | Average vehicle speed
--- | --- | --- | --- | ---
U.K. specs. |  |  |  |
Except U.K. specs. |  |  |  |