#
VARIABLE SWIRL SHUTTER VALVE SWITCH CONSTRUCTION/OPERATION [L3]

id0140b6174400
• The variable swirl shutter valve switch is built into the variable swirl shutter valve actuator.

1 | Variable swirl shutter valve switch

• The output voltage characteristic of the variable swirl shutter valve switch is as shown in the figure.

1 | Variable swirl shutter valve angle (°)
2 | Open: 0
3 | 40-52
4 | 45-57
5 | Close: 64-66
6 | Output voltage (V)
7 | Approx. 5.0
8 | Less than 0.4