#
JOINT SHAFT ASSEMBLY [MZR-CD (RF Turbo)]

id0313008011j5

1. Assemble in the order indicated in the figure.

1 | Bracket
2 | Snap ring (outer side)
3 | Bearing (See Bearing Assembly Note)
4 | Dust seal (differential side) (See Dust Seal (Differential Side) Assembly Note)
5 | Joint shaft (See Joint Shaft Assembly Note)
6 | Snap ring (inner side)
7 | Dust seal (wheel side) (See Dust Seal (Wheel Side) Assembly Note)

## Bearing Assembly Note

1. Install the new bearing using the SSTs.

  Caution

  • Applying excessive force to the bearing could deform the snap ring. Be careful when assembling the bearing.

## Dust Seal (Differential Side) Assembly Note

1. Apply grease to the new dust seal lip.

2. Install the new dust seal (differential side) using a steel plate and the SSTs.

## Joint Shaft Assembly Note

1. Assemble the joint shaft using a press and the SST.

## Dust Seal (Wheel Side) Assembly Note

1. Apply grease to the new dust seal lip.

2. Install the new dust seal (wheel side) using the SSTs.