#
DIFFERENTIAL DISASSEMBLY

id051500802500

1. Disassemble in the order indicated in the table.

1 | Roll pin
2 | Pinion shaft
3 | Pinion gear
4 | Thrust washer
5 | Side gear
6 | Thrust washer
7 | Bearing (side opposite ring gear) (See Bearing (Side Opposite Ring Gear) Disassembly Note.)
8 | Bearing (ring gear side) (See Bearing (Ring Gear Side) Disassembly Note.)
9 | Ring gear and gear case component

## Bearing (Side Opposite Ring Gear) Disassembly Note

1. Remove the bearing using the SSTs.

## Bearing (Ring Gear Side) Disassembly Note

1. Remove the bearing using the SST.