#
CENTER PANEL MODULE REMOVAL/INSTALLATION

id092000804600

1. Cancel the anti-theft operation. (with anti-theft system) (See ANTI-THEFT SYSTEM.)

2. Disconnect the negative battery cable.

3. Remove the glove compartment.

4. Remove the rear console.

5. Remove in the order indicated in the table.

1 | Dial (manual A/C only)
2 | Screw (manual A/C only)
3 | Screw
4 | Bolt
5 | Center panel module (See Center Panel Module Removal Note)
6 | Connector
7 | Antenna feeder

6. Install in the reverse order of removal.

  Caution

  • Make certain that the wiring harness and antenna feeder are not caught between the unit and dashboard. If the harness or the antenna feeder is caught between the unit and dashboard, it may cause trouble or malfunctions.

7. Operate the anti-theft system by setting the code number. (with anti-theft system) (See ANTI-THEFT SYSTEM.)

## Center Panel Module Removal Note

1. Pull the center panel module toward you, then disengage clip A from the dashboard, and remove the center panel module.