#
WATER PUMP CONSTRUCTION/OPERATION [MZR-CD (RF Turbo)]

id0112f1100400

## Construction

• A pressed impeller has been adopted for improved efficiency and reduction in size and weight.
• A highly reliable integrated water seal has been adopted.
• The water pump cannot be disassembled.

1 | External view
2 | Water pump pulley
3 | Water pump body
4 | Sectional view
5 | Impeller

## Operation

• The water pump is driven by the timing belt.