#
VEHICLE SPEEDOMETER SENSOR (VSS) REMOVAL/INSTALLATION [JA5AX-EL]

id051705265200

1. Remove the automatic transaxle. (See AUTOMATIC TRANSAXLE AND TRANSFER REMOVAL/INSTALLATION [JA5AX-EL].)

2. Remove the VSS sensor. (See Automatic Transaxle Workshop Manual JA5A-EL.)

3. Install the VSS sensor. (See Automatic Transaxle Workshop Manual JA5A-EL.)

4. Install the automatic transaxle. (See AUTOMATIC TRANSAXLE AND TRANSFER REMOVAL/INSTALLATION [JA5AX-EL].)