#
SECONDARY SHAFT (NO.1) COMPONENTS DISASSEMBLY

D6E051517040105

1. Disassemble in the order shown in the figure.

1 | Snap ring
2 | Rear bearing (See Rear Bearing and 3rd Gear Disassembly Note.)
3 | 3rd gear (See Rear Bearing and 3rd Gear Disassembly Note.)
4 | Spacer
5 | 3rd needle bearing
6 | 3rd inner ring
7 | 3rd middle ring
8 | 3rd synchronizer ring
9 | Snap ring
10 | 3rd/4th clutch hub component (See 3rd/4th Clutch Hub Component and 4th Gear Disassembly Note.)
11 | Clutch hub sleeve
12 | Steel ball
13 | Spring
14 | Synchronizer key
15 | Clutch hub
16 | 4th synchronizer ring
17 | 4th middle ring
18 | 4th inner ring
19 | 4th gear (See 3rd/4th Clutch Hub Component and 4th Gear Disassembly Note.)
20 | 4th needle bearing
21 | Spacer
22 | Snap ring
23 | 2nd bearing inner race
24 | 2nd needle bearing
25 | 2nd gear
26 | Steel ball
27 | 2nd inner ring
28 | 2nd middle ring
29 | 2nd synchronizer ring
30 | 1st/2nd clutch hub component (See 1st/2nd Clutch Hub Component and 1st Gear Disassembly Note.)
31 | Clutch hub sleeve
32 | Steel ball
33 | Spring
34 | Synchronizer key
35 | Clutch hub
36 | 1st synchronizer ring
37 | 1st middle ring
38 | 1st inner ring
39 | 1st gear (See 1st/2nd Clutch Hub Component and 1st Gear Disassembly Note.)
40 | 1st needle bearing
41 | Secondary shaft (No.1)
42 | Snap ring
43 | Front bearing inner race (See Front Bearing Inner Race Disassembly Note.)

## Rear Bearing and 3rd Gear Disassembly Note

1. Remove the 3rd gear and rear bearing at the same time using the SSTs.

## 3rd/4th Clutch Hub Component and 4th Gear Disassembly Note

1. Remove the 4th gear and 3rd/4th clutch hub component at the same time using the SSTs and a press.

## 1st/2nd Clutch Hub Component and 1st Gear Disassembly Note

1. Remove the 1st gear and 1st/2nd clutch hub component at the same time using the SSTs and a press.

## Front Bearing Inner Race Disassembly Note

1. Remove the front bearing inner race using the SSTs and a press.