#
IGNITION KEY ILLUMINATION OPERATION

id091800101400

## Illumination Condition

• The ignition key illumination glows under all of the following conditions:

  - Driver-side door is open. (Driver-side switch is on.)
  - Ignition switch is in the LOCK or ACC position. (IG off)

## Cancel Condition

• The ignition key illumination goes out under any of the following conditions:

  - 15 s have elapsed since the driver's door was closed (After driver's door switch is on).
  - Ignition switch is in the ON position. (IG on)
  - With all the doors closed, a lock signal from the keyless entry is received.

- Approx. 30 min have elapsed since the driver's door open (Driver's door switch is off)