#
JET PUMP (TRANSFER) OPERATION [L3 4WD]

id0114b11513b3
• The fuel jet pump (venturi) is installed in the return passage from the pressure regulator, and fuel in the fuel tank is pumped to the left side from the right side using the vacuum generated in the passage.
• When the return fuel pressure exceeds a specified value, the relief valve is opened. The relief valve delivers the return fuel directly to the reserve cup. In this way, pressure of the return fuel passing through the fuel jet pump is kept constantly below the specified value.

.

1 | Fuel pump unit
2 | Jet pump (transfer)
3 | Fuel injector
4 | Fuel tank (left side)
5 | Fuel tank (right side)
6 | Fuel flow
7 | Pumped fuel flow