#
CLUTCH HOUSING AND TRANSAXLE CASE COMPONENTS ASSEMBLY [TYPE B]

id051500803813

1. Assemble in the order indicated in the table.

1 | Oil passage
2 | Oil seal (differential) (See Oil Seal (Differential) Assembly Note.)
3 | Adjustment shim
4 | Bearing race (differential) (See Bearing Race (Differential) Assembly Note.)
5 | Adjustment shim
6 | Bearing race (transaxle case) (See Bearing Race (Transaxle Case) Assembly Note.)
7 | Drain plug and washer
8 | Bearing race (differential) (See Bearing Race (Differential) Assembly Note.)
9 | Oil seal (differential) (See Oil Seal (Differential) Assembly Note.)
10 | Hole cover
11 | Breather
12 | Breather cover component
13 | Guide plate
14 | Funnel
15 | Bearing race (secondary shaft)
16 | Oil seal (primary shaft) (See Oil Seal (Primary Shaft) Assembly Note.)
17 | Bearing race (primary shaft)
18 | Oil seal
19 | Spring and washer
20 | Key
21 | Control end
22 | Shift lever shaft
23 | Dust boot
24 | Shift lever
25 | Spring pin
26 | Selector lever
27 | Bracket
28 | Snap ring
29 | Dust boot

## Oil Seal (Differential) Assembly Note

1. Apply transaxle oil to the new oil seal lip.

2. Install the oil seal using the SST.

## Bearing Race (Differential) Assembly Note

1. Install the adjustment shim(s) and install the bearing race using the SST.

## Bearing Race (Transaxle Case) Assembly Note

1. Install the adjustment shim(s) and install the bearing race using the SST.

Primary shaft side

Secondary shaft side

## Oil Seal (Primary Shaft) Assembly Note

1. Apply transaxle oil to outer circumference of the oil seal.

2. Install the new oil seal using the SST.