#
MONITORING SYSTEM AND CONTROL SYSTEM DEVICE RELATIONSHIP CHART [L8, LF, L3]

id0102a1800200
x: Applicable

Component |  |  |  |  |
--- | --- | --- | --- | --- | ---
Input
Battery |  | x |  | x |
Ignition switch | x | x |  |  |
A/C switch, refrigerant pressure switch (high, low pressure) |  |  |  |  |
TP sensor | x |  | x | x | x
ECT sensor | x | x | x | x | x
IAT sensor | x |  | x |  | x
MAF sensor | x | x | x | x | x
A/F sensor | x | x | x |  | x
HO2S | x | x | x |  | x
Fuel gauge sender unit |  |  |  |  |
MAP sensor |  |  |  |  |
CMP sensor |  |  |  | x |
CKP sensor | x | x | x | x | x
VSS | x |  |  | x |
Output
Fuel injector |  |  |  |  | x
A/F sensor heater |  | x |  |  |
HO2S heater |  | x |  |  |
EGR valve |  |  |  |  |
Purge solenoid valve | x |  | x |  | x
EVAP system leak detection pump |  |  |  |  |
MIL | x | x | x | x | x
DLC-2 | x | x | x | x | x