#
SECURITY ACCESS PROCEDURE

id0914z6810300

1. Connect the WDS or equivalent to the DLC-2.

2. Select "BODY/SECURITY/PATS (immobilizer) function" from the WDS or equivalent screen menu.

3. Select the items to be performed from the following:

  • Additional card key programming
  • Card key ID number clearing
  • Steering lock unit programming
  • Ignition key additional programming (with immobilizer system)
  • Ignition key ID number clearing (with immobilizer system)
  • Customer spare key programming enable (with immobilizer system)
  • Customer spare key programming disable (with immobilizer system)

4. The security access begins and the WDS or equivalent displays the "OUT-CODE".

  Note

  • When "OUT-CODE" is first displayed, turning the ignition switch from the LOCK to the ON position 5 times will change the "OUT-CODE".

5. Input "IN-CODE" corresponding to "OUT-CODE" displayed on the WDS or equivalent screen.

6. If the security access is successful, selected item can be performed.