#
WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION

id091900474600

  Warning

• When the ignition switch is turned to the ON position, and the wiper and washer switch is in the AUTO position, the windshield wipers may operate automatically in the following cases. Always turn the ignition switch, and the wiper and washer switch off before handling the windshield wipers; otherwise a pinched hand or fingers could result in injury or a wiper system malfunction:

- The upper part of the windshield rain sensor is touched.

- The windshield receives an impact.

- The rain sensor receives an impact from the cabin.

1. Remove in the order indicated in the table.

1 | Cap
2 | Nut
3 | Windshield wiper arm (See Windshield Wiper Arm Installation Note.)
4 | Windshield wiper blade
5 | Rubber brush

2. Install in the reverse order of removal.

3. Adjust the windshield wiper arm and blade. (See WINDSHIELD WIPER ARM AND BLADE ADJUSTMENT.)

## Windshield Wiper Arm Installation Note

1. Clean the windshield wiper arm connector shafts using a wire brush before installing the windshield wiper arms.