#
CLIMATE CONTROL UNIT CONSTRUCTION [FULL-AUTO AIR CONDITIONER]

id0740001009a1
• A logic-type climate control unit is used with the full-auto air conditioner.
• The temperature setting dial, fan switch have been enlarged to improve ease of operation.
• The A/C, REC/FRESH and rear defroster switches equipped in the current climate control unit have been relocated to the center panel.

.

1 | Climate control unit
2 | Fan switch
3 | OFF switch
4 | MODE switch
5 | Temperature setting dial
6 | Defroster switch
7 | AUTO switch

• Information about the operating condition of the system is displayed on the information display.

.

1 | Information display