ON‐BOARD DIAGNOSTIC WIRING DIAGRAM [L3 Turbo]

id0102b7122200

d6e140bt7003

1 | IAT sensor
2 | MAF sensor
3 | APP sensor
4 | Fuel pressure sensor
5 | ECT sensor
6 | MAP sensor
7 | Boost air temperature sensor
8 | HO2S
9 | A/F sensor
10 | Injector driver module
11 | Fuel injector No.1
12 | Fuel injector No.2
13 | Fuel injector No.3
14 | Fuel injector No.4
15 | Injector driver relay
16 | A/F sensor heater
17 | HO2S heater
18 | Fan control module
19 | Fan relay (Main)
20 | A/C relay
21 | Fuel pump speed control relay
22 | Fuel pump resistor
23 | Fuel pump
24 | Fuel pump relay
25 | Main relay
26 | Starter relay
27 | Ignition switch
28 | Battery

d6e140bt7004

29 | CKP sensor
30 | CMP sensor
31 | Brake light
32 | Brake switch
33 | Variable swirl shutter valve switch
34 | A/C switch
35 | Refrigerant pressure switch (High and low)
36 | Refrigerant pressure switch (Middle)
37 | PSP switch
38 | Neutral switch
39 | CPP switch
40 | Cruise control switch
41 | Generator
42 | TP sensor
43 | Drive-by-wire-relay
44 | EGR valve
45 | Purge solenoid valve
46 | Wastegate control solenoid valve
47 | Variable swirl solenoid valve
48 | Spill valve control solenoid valve (High pressure fuel pump)
49 | Instrument cluster
50 | Coil (Immobilizer system)
51 | Ignition coil No.1
52 | Ignition coil No.2
53 | Ignition coil No.3
54 | Ignition coil No.4
55 | Generator (Field coil)
56 | Throttle actuator