#
CONTROL SYSTEM LOCATION INDEX [L8, LF, L3]

id0140a5804100

.

1 | MAF/IAT sensor (See INTAKE AIR TEMPERATURE (IAT) SENSOR INSPECTION [L8, LF, L3].) (See MASS AIR FLOW (MAF) SENSOR INSPECTION [L8, LF, L3].)
2 | TP sensor (See THROTTLE POSITION (TP) SENSOR INSPECTION [L8, LF, L3].)
3 | MAP sensor (See MANIFOLD ABSOLUTE PRESSURE (MAP) SENSOR INSPECTION [L8, LF, L3].)
4 | ECT sensor (See ENGINE COOLANT TEMPERATURE (ECT) SENSOR REMOVAL/INSTALLATION [L8, LF, L3].) (See ENGINE COOLANT TEMPERATURE (ECT) SENSOR INSPECTION [L8, LF, L3].)
5 | CKP sensor (See CRANKSHAFT POSITION (CKP) SENSOR INSPECTION [L8, LF, L3].) (See CRANKSHAFT POSITION (CKP) SENSOR REMOVAL/INSTALLATION [L8, LF, L3].)
6 | CMP sensor (See CAMSHAFT POSITION (CMP) SENSOR INSPECTION [L8, LF, L3].)
7 | Knock sensor (See KNOCK SENSOR (KS) INSPECTION [L8, LF, L3].) (See KNOCK SENSOR (KS) REMOVAL/INSTALLATION [L8, LF, L3].)
8 | A/F sensor, HO2S (See AIR FUEL RATIO (A/F) SENSOR, HEATED OXYGEN SENSOR (HO2S) INSPECTION [L8, LF, L3].)
9 | PSP switch (See POWER STEERING PRESSURE (PSP) SWITCH INSPECTION [L8, LF, L3].)
10 | Clutch pedal position (CPP) switch (MTX) (See CLUTCH PEDAL POSITION (CPP) SWITCH INSPECTION [L8, LF, L3].)
11 | Neutral switch (MTX) (See NEUTRAL SWITCH INSPECTION [L8, LF, L3].)
12 | PCM (See PCM INSPECTION [L8, LF, L3].)
13 | Accelerator pedal position (APP) sensor (See ACCELERATOR PEDAL REMOVAL/INSTALLATION [L8, LF, L3].)