#
FRONT BRAKE (DISC) CONSTRUCTION [AUSTRALIAN, GENERAL (L.H.D. R.H.D.) SPECS.]

id0411001004c4
4SD (except L3 Turbo), 5HB, WGN (except Australian specs.)
• Large diameter, ventilated disc type front brakes with a 274 mm {10.8 in} diameter and 24 mm {0.945 in} thickness have been adopted, improving braking force and fade resistance.
WGN (Australian specs.)
• Large diameter, ventilated disc type front brakes with a 283 mm {11.1 in} diameter and a 25 mm {0.984 in} thickness have been adopted, improving braking force and fade resistance.

4SD (L3 Turbo)
• Large diameter, ventilated disc type front brakes with a 320 mm {12.6 in} diameter and a 25 mm {0.984 in} thickness have been adopted, improving braking force and fade resistance.