#
INTRUDER SENSOR REMOVAL/INSTALLATION [WGN]

id0914z68094a6

## Front Intruder Sensor (With Sliding Sunroof)

• There are no changes from the current front intruder sensor removal/installation procedure.

## Center Intruder Sensor (Without Sliding Sunroof)

• There are no changes from the current center intruder sensor removal/installation procedure.

## Rear Intruder Sensor

1. Disconnect the negative battery cable.

2. Remove the headliner.

3. Remove in the order indicated in the table.

1 | Connector
2 | Screw
3 | Rear intruder sensor

4. Install in the reverse order of removal.