#
JOINT SHAFT DISASSEMBLY [L3 Turbo]

id0313008010b5

1. Disassemble in the order indicated in the table.

1 | Dust seal (See Dust Seal Disassembly Note)
2 | Snap ring
3 | Snap ring
4 | Joint shaft (See Joint Shaft Disassembly Note)
5 | Bearing
6 | Bracket

## Dust Seal Disassembly Note

1. Remove the dust seal using a flathead screwdriver.

## Joint Shaft Disassembly Note

1. Remove the joint shaft as shown in the figure.