#
FUEL TEMPERATURE SENSOR CONSTRUCTION/OPERATION [MZR-CD (RF Turbo)]

id0140f1181800
• Installed to the supply pump.
• The thermistor type fuel temperature sensor changes resistance according to the fuel temperature.
• The resistance decreases if the fuel temperature increases and, conversely, increases if the fuel temperature decreases.

1 | Thermistor
2 | Fuel temperature sensor
3 | Fuel temperature sensor characteristic
4 | Fuel temperature
5 | Resistance
6 | Large
7 | Small
8 | High
9 | Low