DIESEL PARTICULATE FILTER REGENERATION CONTROL BLOCK DIAGRAM [MZR-CD (RF Turbo)]

id0140f1222900

g6e140ct2014

1 | Clutch switch
2 | Neutral switch
3 | PSP switch
4 | APP sensor
5 | MAF/IAT sensor
6 | IAT sensor No.2
7 | ECT sensor
8 | BARO sensor (integrated in PCM)
9 | Boost sensor
10 | Fuel pressure sensor
11 | CKP sensor
12 | Vehicle speed signal
13 | Exhaust gas pressure sensor
14 | Exhaust gas pressure correction temperature sensor
15 | Exhaust gas temperature sensor (upper)
16 | Exhaust gas temperature sensor (middle)
17 | Exhaust gas temperature sensor (lower)
18 | Intake shutter valve position sensor
19 | EGR valve position sensor
20 | A/F sensor
21 | Fuel injector
22 | EGR valve
23 | Intake shutter valve
24 | Glow plug relay