#
FUEL PRESSURE SENSOR CONSTRUCTION/OPERATION [L3 Turbo]

id0140b6104600

  Note

  • When the fuel pressure sensor replaces, replace a new fuel delivery pipe with a new fuel pressure sensor.

• Installed to the end of the fuel delivery pipe.

1 | Fuel injector
2 | Fuel pressure sensor
3 | Fuel delivery pipe

• When pressure is applied to the piezoelectric element in the sensor, an electric potential difference occurs.
• Output voltage increases ad the fuel pressure increases.

1 | Fuel pressure sensor
2 | Fuel pressure sensor characteristic
3 | High
4 | Out put voltage
5 | Fuel pressure