#
DRIVE BELT CONSTRUCTION [MZR-CD (RF Turbo)]

id0110f1102500

## Structure

• The serpentine type drive belt uses a V-ribbed belt to drive the supplemental units. This shortens the length of the engine and makes it easier to service.
• A front drive belt auto tensioner with an embedded coil spring has been adopted for drive belt tension. The tensioner pulley automatically maintains drive belt tension.

1 | Drive belt
2 | Auto tensioner