#
DTC B1342

id0902j0839600

DTC B1342 | ECU is faulted
--- | ---
DETECTION CONDITION | BCM microcomputer malfunction
POSSIBLE CAUSE | • BCM microcomputer malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT DTC • Clear the DTC from the BCM memory using the WDS or equivalent. • Is the same DTC present? | Yes | Replace the BCM. (See BODY CONTROL MODULE (BCM) REMOVAL/INSTALLATION.)
No | DTC troubleshooting completed.