ENGINE CONTROL SYSTEM DIAGRAM [MZR-CD (RF Turbo)]

id0140f1100300

g6e140ct1503

1 | Air cleaner
2 | Vacuum chamber
3 | VBC check valve
4 | MAF/IAT sensor
5 | VBC solenoid valve
6 | Vacuum damper
7 | Guide blade actuator
8 | Turbocharger
9 | Charge air cooler
10 | IAT sensor No.2
11 | Boost sensor
12 | EGR valve
13 | EGR cooler
14 | Fuel tank
15 | Fuel filter
16 | Fuel warmer
17 | Supply pump
18 | Suction control valve
19 | Fuel temperature sensor
20 | Common rail
21 | Fuel pressure sensor
22 | Fuel pressure limiter
23 | Glow plug
24 | Fuel injector
25 | ECT sensor
26 | CMP sensor
27 | Oxidation catalytic converter
28 | Diesel particulate filter
29 | Exhaust gas pressure sensor (with exhaust gas pressure correction temperature sensor)
30 | Exhaust gas temperature sensor (upper)
31 | Exhaust gas temperature sensor (middle)
32 | Exhaust gas temperature sensor (lower)
33 | Main silencer
34 | Vacuum pump
35 | CKP sensor
36 | APP sensor
37 | Glow plug relay
38 | PCM control relay (main relay)
39 | Engine switch
40 | Starter relay
41 | Neutral switch
42 | A/C relay
43 | Clutch switch
44 | CAN bus
45 | PSP switch
46 | Intake shutter valve
47 | Generator
48 | BARO sensor (built into PCM)
49 | A/F sensor
50 | To PCM
51 | Fuel flow