#
SYMPTOM TROUBLESHOOTING CHART [KEYLESS ENTRY SYSTEM]

id0903d2812700

No. | Troubleshooting item | Description | Page
--- | --- | --- | ---
1 | One or more on-board diagnostic functions inoperative | • Malfunction in door lock linkage system | See NO.1 ONE OR MORE ON-BOARD DIAGNOSTIC FUNCTIONS INOPERATIVE [KEYLESS ENTRY SYSTEM]
2 | All on-board diagnostic functions inoperative | • Malfunction in BCM power supply circuit, door latch switch circuit, BCM ground circuit, or keyless receiver. | See NO.2 ALL ON-BOARD DIAGNOSTIC FUNCTIONS INOPERATIVE
3 | Transmitter ID code cannot be reprogrammed | • Malfunction in transmitter battery, transmitter, keyless receive bracket, keyless receive bracket ground screw, or BCM circuit. keyless receive circuit. | See NO.3 TRANSMITTER ID CODE CANNOT BE REPROGRAMMED [KEYLESS ENTRY SYSTEM]