#
NO.1 MELTING OF MAIN OR OTHER FUSES [L8, LF, L3]

id0103a1800700

1 | MELTING OF MAIN OR OTHER FUSES
--- | ---
[TROUBLESHOOTING HINTS] Inspect condition of fuse.

Damaged fuse | Related wiring harness
--- | ---
MAIN | MAIN fuse • BTN fuse - ROOM fuse • IG KEY2 fuse • FAN fuse • AD FAN fuse
BTN | BTN fuse • ROOM fuse
ROOM | ROOM fuse • DLC-2
IG KEY2 | IG KEY2 fuse • Ignition switch
FAN | FAN fuse • Cooling fan relay No.2
AD FAN | AD FAN fuse • Cooling fan relay No.1
IG KEY1 | IG KEY1 fuse • Ignition switch - ENGINE fuse
ENGINE | ENGINE fuse • Fuel pump relay • PCM • Ignition coil • Condenser
FUEL PUMP | FUEL PUMP fuse • Main relay - PCM • Fuel pump relay - Fuel pump
ENG +B | ENG +B fuse • PCM
ETC | ETC fuse • ET control relay - PCM
INJ | INJ fuse • ET control relay - PCM • PCM • Fuel injector
ENG BAR | ENG BAR fuse • EGR valve • Purge solenoid valve • MAF/IAT sensor • Oil control valve (LF, L3) • Variable intake-air solenoid valve (LF, L3) • A/F sensor