#
FOREWORD [L8, LF, L3]

id0103a1910000
• When the customer reports a vehicle malfunction, check the malfunction indicator lamp (MIL) indication and diagnostic trouble code (DTC), then diagnose the malfunction according to the following flowchart:

  - If a DTC exists, diagnose the applicable DTC inspection. (See DTC TABLE [L8, LF, L3].)
  - If no DTC exists and the MIL does not illuminate or flash, diagnose the applicable symptom troubleshooting. (See QUICK DIAGNOSTIC CHART [L8, LF, L3].)

*: Malfunction Indicator Lamp (MIL), Generator Warning Light, Security Light