#
WHEEL HUB BOLT REPLACEMENT [4WD]

id0312008008a2

1. Remove the brake caliper component and the disc plate.

2. Remove the wheel hub bolt using the SST as shown in the figure.

  Note

  • If the dust cover interferes with the wheel hub bolt and the wheel hub bolt cannot be removed, tap the part shown in the figure with a chisel lightly and bend the process back to the knuckle side.

3. Install a new wheel hub bolt into the wheel hub and install a washer and hub nut on the hub bolt.

4. Tighten the hub nut while holding the wheel hub using a brass bar.